{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"merged":[[0,0,0,7],[1,0,1,7],[2,0,2,2],[3,1,3,2],[4,0,4,7],[5,0,5,7],[6,0,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,0,14,7],[22,0,22,7],[27,0,27,7],[32,0,32,6],[37,0,37,7],[47,0,47,4]]}
["弱电设备采购清单"]
["一、LED屏 "]
["货物名称",null,null,"屏体尺寸","数量","单位","单价（元）","小计（元）"]
[1,"P2.5室内全彩显示屏",null,"2985*1705",5.07,"平方"]
["备注：报价中包含屏体框架、视频处理器、发送卡、接收卡和无线投屏器、配套辅料以及安装调试。"]
["二、电视及宣誓厅音箱设备清单"]
["货物名称",null,null,"规格或型号","数量","单位","单价（元）","小计（元）"]
[1,"VR及游戏65寸电视",null,"65寸",4,"台"]
[2,"拍照签名系统电视",null,"65寸",1,"台"]
[3,"服务大厅吊装电视",null,"65寸",1,"台"]
[4,"宣誓电视",null,"43寸",1,"台"]
[5,"宣誓厅功放及4只天花喇叭",null,"150w及以上，喇叭6W及以上",1,"套"]
[6,"安装支架",null,"吊装3m可伸缩",1,"套"]
[7,"安装支架",null,"壁装",6,"套"]
["三、投影系统设备清单"]
["序号 ","设备或材料名称 ","规格 ","单位","数量 ","单价（元）","小计","备注"]
[1,"幕布","100寸，4:3，自动幕布","套",2]
[2,"投影机","1.亮度：3200流明；2.分辨率：1920*1080； 3.投影光源：高压汞灯灯泡； 4.显示技术：3LCD","台",2]
[5,"专用吊架","加厚","套",1]
[6,"喇叭","6W及以上","只",4]
[7,"功放","150w及以上","只",2]
[8,"落地机柜 ","22U","台",2]
["四、签名拍照系统清单"]
["序号","产品名称","参数说明","数量","单位","单价","金额","备注"]
[1,"21.5寸触摸一体机","尺寸：21.5寸壁挂触摸一体机\n触摸：红外十点触摸\n主机配置：I5四代独立CPU+8G内存+128G固态硬盘",1,"台"]
[2,"摄像头","高清USB拍照摄像机",1,"台",null,null,"1.USB接口2.清晰度大于等于720P"]
[3,"触控互动系统软件V1.0","1、倒计时拍照功能；\n2、签名功能；\n3、可根据自己喜欢选取拍照相框背景；\n4、微信扫二维码下载、保存照片；        5、留言功能；                                6、当日和区间签名拍照人数统计功能；\n7、打印照片。（需单独配打印机）",1,"套"]
["五、网络设备清单"]
["序号 ","设备或材料名称 ","规格 、品牌","单位","数量 ","单价（元）","小计","备注"]
[1,"48口交换机","千兆","台",1]
[2,"无线路由器","1.传输速率：2.4GHz：300Mbps  5GHz：867Mbps         2.频率范围：双频（2.4GHz，5GHz）","台",2]
[3,"落地机柜 ","22U","台",1]
["六、网络布线系统设备清单"]
["序号 ","设备或材料名称 ","规格 、品牌","单位","数量 ","单价（元）","小计","备注"]
[1,"模块","超五类","个",32]
[2,"面板","双口86面板","个",32]
[3,"落地机柜 ","22U","台",1]
["七、汇总报价"]
["序号","项目名称","金额","备注"]
[1,"LED屏"]
[2,"电视及宣誓厅音箱设备"]
[3,"投影系统设备"]
[4,"签名拍照系统"]
[5,"网络设备及网络布线系统"]
[6,"施工调试费"]
[7,"税费"]
[6,"含税总价"]
["注：以上清单作为本次采购的基础清单，具体内容须根据甲方现场实际需求进行调整。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}